// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca953x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "glinet,gl-xe300", "qca,qca9531";
	model = "GL.iNet GL-XE300";

	aliases {
		label-mac-device = &eth0;
	};

	gpio-export {
		compatible = "gpio-export";

		gpio_lte_power {
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
			gpio-export,name = "lte_power";
			gpio-export,output = <1>;
		};

		gpio_sd_detect {
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			gpio-export,name = "sd_detect";
			gpio-export,output = <0>;
		};
	};

	keys {
		compatible = "gpio-keys";

		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		lan {
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_GREEN>;
		};

		wan {
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_GREEN>;
		};

		wlan {
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			linux,default-trigger = "phy0tpt";
		};

		lte {
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			label = "green:lte";
		};
	};

	i2c_gpio: i2c@0 {
		compatible = "i2c-gpio";
		gpios = <&gpio 15 GPIO_ACTIVE_HIGH
		         &gpio 4  GPIO_ACTIVE_HIGH>;
		i2c-gpio,delay-us = <5>;
		i2c-gpio,timeout-ms = <100>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "okay";
	};
};

&pcie0 {
	status = "okay";
};

&usb0 {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
			};

			partition@50000 {
				label = "art";
				reg = <0x50000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_art_0: macaddr@0 {
						compatible = "mac-base";
						reg = <0x0 0x6>;
						#nvmem-cell-cells = <1>;
					};

					cal_art_1000: calibration@1000 {
						reg = <0x1000 0x440>;
					};
				};
			};

			partition@60000 {
				label = "kernel";
				reg = <0x60000 0x400000>;
			};

			partition@460000 {
				label = "nor_reserved";
				reg = <0x460000 0xba0000>;
			};
		};
	};

	flash@1 {
		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ubi";
				reg = <0x0 0x8000000>;
			};
		};
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy4>;

	nvmem-cells = <&macaddr_art_0 0>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	nvmem-cells = <&macaddr_art_0 1>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	status = "okay";

	nvmem-cells = <&cal_art_1000>;
	nvmem-cell-names = "calibration";
};

